Assignment #4

Circuit Modeling

ELEC 4700

Modelling of Integrated Devices

By:

**Konrad Socha 101037642**

Departments of Electronics

Carleton University

[konradsocha@cmail.carleton.ca](mailto:konradsocha@cmail.carleton.ca)

Q1.

Chart, line chart

Description automatically generated

Fig1. Current Plot

Q2.

The linear fit gives a resistance of R3 = 2.125770e-01

Q3.

a)i)

Eq1. Iin – G1(V1-V2) – C\*d(V1-V2)/dt = 0

Eq2. G1(V1-V2) + C\*d(V1-V2)/dt -V2\*G2 - Il= 0

Eq3. Il – G3\*V3 = 0

Eq4. I4 – G4\*(V4-V5) = 0

Eq5. G4\*(V4-V5) – G0 \*V0 = 0

Eq6. dIl = dt(V2-V3)/L

Eq7. Vin = Vout

Eq8. V4 = I3\*alpha

a)ii)

Eq1. V1\*(-G1); V2\*(G1); Iin;

Eq2. V1(G1); V2(-G1 + -G2); -Il;

Eq3. V3(-G3); Il;

Eq4. V4(-G4); V5(G4); I4;

Eq5. V4(G4); V5(G5);

Eq6. -L; V2 -V3;

Eq7. Vin; V1;

Eq8. V4; V3(-alpha\*G3);

a)iii)

A picture containing table

Description automatically generated

Fig 2. Matrices for C G and F

b) i)

Chart, line chart

Description automatically generated

Fig 3. DC Sweep

b)ii)

Chart, line chart

Description automatically generated

Fig 4. AC Sweep

b)iii)

Chart, histogram

Description automatically generated

Fig 5. Vout Histogram

Chart, histogram

Description automatically generated

Fig 6. Capacitance Histogram

Q4. a) This circuit seems to function as a LPF as seen in figure 4.

b) Low frequencies will result in a gain of approximately 40db with a drop at higher frequencies approaching -40db when angular frequency is greater than 500rad/s.

c) C(dV/dt) + GV = F

C \* (Vn / dt) – C (Vn -1 / dt) + G \* Vn = F(t)

d)

ii)a)

iii)

Chart

Description automatically generated

Fig 7. Step Response Transient

iv)

Chart

Description automatically generated

Fig 8. Step Response Fourier

ii)b)

iii)

Chart, bar chart, histogram

Description automatically generated

Fig 9. Sine Response Transient

iv)

Chart

Description automatically generated

Fig 9. Sine Response Fourier

ii)c)

iii)

Chart, line chart

Description automatically generated

Fig 10. Gaussian Response Transient

iv)

Chart, histogram

Description automatically generated

Fig 10. Gaussian Response Fourier

d) v) The time step reduction causes the transient response to be greatly altered. In the case below the response only rises there is no peak or drop even though the simulated time is the same.

Chart, line chart

Description automatically generated

Fig 7. Step Response Transient with reduced timestep